**Changing PRO-view cameras to DHCP**

1. Download our IP Camera search tool from the link below and install
<https://drive.google.com/open?id=0B9Cfm4XKkkp8alRCY3BFUlZoYlU>
2. Connect a laptop into a numbered port on the NVR. You may need to remove a camera.
3. Once everything is connected, run the IP camera search tool on your laptop and click search at the bottom. This should show all the connected cameras.

**If this shows no cameras, plug your laptop into the LAN on the NVR**



1. Select the camera you want to make DHCP, on the right hand side tick the “DHCP Enable” box then enter the username and password.
Username: admin
Password: admin
Once entered, press modify and a box will pop up saying “Modify Success”, this will reboot the camera. Once done, it will now be on a DHCP address and display on screen.